**Reuse of greywater**

**1Hanan A. Fouad, 1Rehab M. Elhefny, 2Hanna F. Habeb**

*1Sanitary & Environmental Engineering, Faculty of Engineering at Shoubra, Benha University, Egypt*

*2Civil Engineering Department, Higher Institute of Engineering, 15th May City, Egypt*

|  |
| --- |
| Received 11 October 2016; Accepted 22 January 2017; Available online 26 January 2017 **Address For Correspondence:** Hanan A. Fouad, Sanitary & Environmental Engineering, Faculty of Engineering at Shoubra, Benha University, Egypt  |

|  |
| --- |
|  **ABSTRACT** Greywater is the wastewater resulted in houses through the use of water for laundry and bathroom. This research aims to treat and reuse greywater for agriculture, toilet flushing, and street washing. The treatment system consists of collection tank followed by sedimentation unit and three consecutive filters consisting of different materials such as (gravel, plastic balls, crushed stones, and gravel sand). A dose of chlorine and alum were added to the best sample and tested. (pH, BOD, COD,DO, total suspended solids, and alkalinity) were measured. Samples were tested at three different rates. Results have shown that sand and gravel is the best filter media among the used materials, the best flow rate was 0.0226 l/sec. **KEYWORDS:** Greywater Treatment, Recycling, Alum, Chlorine Dose.  |