Highlights

* Novel numerical simulation technique for Stand alone Nanofluid Photovoltaic thermal systems.
* AlooH, Al2O3 and MWCNTs Nanofluid were simulated in different systems
* Results showed a very good a greement between the numerical and experimental results.
* Furthermore, improved exergy analysis model is provided with sustainability assessment.